The pictures illustrate different steps towards production of leather commodities. It is clear that there are 10 steps in the process, from initial drying animal skin to the final step of producing leather goods.

At the first step to the production of leather goods, skins of animal are peel off and then they are dried. next, dried skins are transported to the leather factories by truck in order to be washed in the containers including the solution of water and lime. Afterwards, skins are soaked in the chemical liquid, lime, only.

At the step six of this process, animal’s skins are got thin by pressure of cylindrical machine and finally become flattening, so that they are soaked in the tannic acid which contains water and vegetable matter. Furthermore, these materials are polished up to be shiny and smooth. At the final steps, the leathers taken out to the leather shops as the end product: shoes, bags and so on.