The diagram illustrates the production of the leather goods through 11 steps starting from drying the material till the production of bags and shoes.

At the beginning, animal skin is dried under the heat of sun.after that it is transported to factory by truck where this material is washed using a mixture of lime and water. in subsequencent stage, it is soaked in lime.Afterwards, the ingredient is gone through a special machine to be flatten.

in the next step,The result later on will be flattened and be put into a container that consists of different mixtures, such as: water and vegetable matter. After a period of time of the soaking process, the skin will eventually be polished and assembled into some kind of leather goods, for example: shoes, handbag and ball.

To sum up, in order to produce the leader goods, there are some important steps in which the second stage takes much longer than others.